Installation for Linux:

To install the Modem Neolec Freeway 56k run 

slmdm-2.7.14-0.i386.rpm for the core package.

After you have done this run: 

slmdm-amr-2.7.14-0.i386.rpm for the PCI-Version or 
slmdm-usb-2.7.14-0.i386.rpm for the USB-Version to install the Modem-Drivers.

To run in Console/Shell type: 	# rpm -i /path/to/slmdm-2.7.14-0.i386.rpm
				# rpm -i /path/to/slmdm-amr-2.7.14-0.i386.rpm or
				# rpm -i /path/to/slmdm-usb-2.7.14-0.i386.rpm

Note: currently you cannot install and use both PCI and USB Modems


Uninstall:

Type in Console/Shell:


1. rpm -e slmdm-amr for the PCI-Version oder 
   rpm -e slmdm-usb for the USB-Version.

2. rpm -e slmdm



The Drivers are testet on following Systems:

Suse Linux 8.2
Suse Linux 9.0
